<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.5.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="37" y2="0" width="0" layer="20"/>
<wire x1="37" y1="0" x2="37" y2="48" width="0" layer="20"/>
<wire x1="37" y1="48" x2="0" y2="48" width="0" layer="20"/>
<wire x1="0" y1="48" x2="0" y2="0" width="0" layer="20"/>
<hole x="3" y="3" drill="2.8"/>
<hole x="3" y="45" drill="2.8"/>
<hole x="34" y="3" drill="2.8"/>
<hole x="34" y="45" drill="2.8"/>
<text>1</text>
<text>USB Keyboard Controller</text>
<text>github.com/thedalles77/USB_Laptop_Keyboard_Controller</text>
</plain>
<libraries>
<library name="Teensy_LC">
<packages>
<package name="TEENSY_LC">
</package>
</packages>
</library>
<library name="oshw">
<description>&lt;p&gt;&lt;strong&gt;Open Source Hardware PCB Logos&lt;/strong&gt;
&lt;p&gt;A simple polygon based version of the OSHWA logos for use on Eagle PCB's
&lt;p&gt;For use please refer to the OSHWA definition at &lt;a href="http://www.oshwa.org/definition/"&gt;http://www.oshwa.org/definition/&lt;/a&gt;
&lt;p&gt;Based on the NBitWonder version (&lt;a href="http://nbitwonder.com"&gt;http://nbitwonder.com&lt;/a&gt;)
&lt;p&gt;&lt;strong&gt;Andrew Cooper&lt;/strong&gt;&lt;br&gt;28Nov2016&lt;br&gt;&lt;a href="http://www.darkerview.com"&gt;www.DarkerView.com&lt;/a&gt;</description>
<packages>
<package name="OSHW_5MM">
</package>
</packages>
</library>
<library name="1.0MM DIP FPC26">
<packages>
<package name="T1200_CON">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="J1" library="1.0MM DIP FPC26" package="T1200_CON" value="1.00MM DIP FPC">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$1" library="Teensy_LC" package="TEENSY_LC" value="TEENSY_LC"/>
<element name="U$2" library="oshw" package="OSHW_5MM" value=""/>
</elements>
<signals>
<signal name="IO_23">
<contactref element="J1" pad="P$1"/>
<contactref element="U$1" pad="23"/>
</signal>
<signal name="IO_0">
<contactref element="J1" pad="P$2"/>
<contactref element="U$1" pad="0"/>
</signal>
<signal name="IO_22">
<contactref element="J1" pad="P$3"/>
<contactref element="U$1" pad="22"/>
</signal>
<signal name="IO_1">
<contactref element="J1" pad="P$4"/>
<contactref element="U$1" pad="1"/>
</signal>
<signal name="IO_24">
<contactref element="J1" pad="P$5"/>
<contactref element="U$1" pad="24"/>
</signal>
<signal name="IO_2">
<contactref element="J1" pad="P$6"/>
<contactref element="U$1" pad="2"/>
</signal>
<signal name="IO_21">
<contactref element="J1" pad="P$7"/>
<contactref element="U$1" pad="21"/>
</signal>
<signal name="IO_3">
<contactref element="J1" pad="P$8"/>
<contactref element="U$1" pad="3"/>
</signal>
<signal name="IO_25">
<contactref element="J1" pad="P$9"/>
<contactref element="U$1" pad="25"/>
</signal>
<signal name="IO_4">
<contactref element="J1" pad="P$10"/>
<contactref element="U$1" pad="4"/>
</signal>
<signal name="IO_20">
<contactref element="J1" pad="P$11"/>
<contactref element="U$1" pad="20"/>
</signal>
<signal name="IO_5">
<contactref element="J1" pad="P$12"/>
<contactref element="U$1" pad="5"/>
</signal>
<signal name="IO_19">
<contactref element="J1" pad="P$13"/>
<contactref element="U$1" pad="19"/>
</signal>
<signal name="IO_6">
<contactref element="J1" pad="P$14"/>
<contactref element="U$1" pad="6"/>
</signal>
<signal name="IO_18">
<contactref element="J1" pad="P$15"/>
<contactref element="U$1" pad="18"/>
</signal>
<signal name="IO_7">
<contactref element="J1" pad="P$16"/>
<contactref element="U$1" pad="7"/>
</signal>
<signal name="IO_17">
<contactref element="J1" pad="P$17"/>
<contactref element="U$1" pad="17"/>
</signal>
<signal name="IO_8">
<contactref element="J1" pad="P$18"/>
<contactref element="U$1" pad="8"/>
</signal>
<signal name="IO_16">
<contactref element="J1" pad="P$19"/>
<contactref element="U$1" pad="16"/>
</signal>
<signal name="IO_9">
<contactref element="J1" pad="P$20"/>
<contactref element="U$1" pad="9"/>
</signal>
<signal name="IO_15">
<contactref element="J1" pad="P$21"/>
<contactref element="U$1" pad="15"/>
</signal>
<signal name="IO_10">
<contactref element="J1" pad="P$22"/>
<contactref element="U$1" pad="10"/>
</signal>
<signal name="GND">
<contactref element="U$1" pad="GND1"/>
<contactref element="U$1" pad="GND2"/>
<contactref element="U$1" pad="GND3"/>
</signal>
<signal name="IO_11">
<contactref element="U$1" pad="11"/>
<contactref element="J1" pad="P$24"/>
</signal>
<signal name="IO_12">
<contactref element="U$1" pad="12"/>
<contactref element="J1" pad="P$26"/>
</signal>
<signal name="IO_14">
<contactref element="U$1" pad="14"/>
<contactref element="J1" pad="P$23"/>
</signal>
<signal name="IO_26">
<contactref element="U$1" pad="26"/>
<contactref element="J1" pad="P$25"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
