<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.5.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="41" y2="0" width="0" layer="20"/>
<wire x1="41" y1="0" x2="41" y2="50" width="0" layer="20"/>
<wire x1="41" y1="50" x2="0" y2="50" width="0" layer="20"/>
<wire x1="0" y1="50" x2="0" y2="0" width="0" layer="20"/>
<hole x="3" y="3" drill="2.8"/>
<hole x="38" y="3" drill="2.8"/>
<hole x="38" y="47" drill="2.8"/>
<hole x="3" y="47" drill="2.8"/>
<text>1</text>
<text>14</text>
<text>13</text>
<text>26</text>
<text>GND</text>
<text>3V</text>
<text>24</text>
<text>23</text>
<text>5V</text>
<text>Info at github.com/thedalles77/
USB_Laptop_Keyboard_Controller</text>
<text>USB Keyboard Controller</text>
<text>Zenith Supersport</text>
<text>U1</text>
</plain>
<libraries>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Connectors&lt;/h3&gt;
This library contains electrically-functional connectors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X08">
<description>&lt;h3&gt;Plated Through Hole -8 Pin&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:8&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_08&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="Teensy_LC">
<packages>
<package name="TEENSY_LC">
</package>
</packages>
</library>
<library name="Zenith">
<packages>
<package name="ZENITH_CON">
</package>
</packages>
</library>
<library name="oshw">
<description>&lt;p&gt;&lt;strong&gt;Open Source Hardware PCB Logos&lt;/strong&gt;
&lt;p&gt;A simple polygon based version of the OSHWA logos for use on Eagle PCB's
&lt;p&gt;For use please refer to the OSHWA definition at &lt;a href="http://www.oshwa.org/definition/"&gt;http://www.oshwa.org/definition/&lt;/a&gt;
&lt;p&gt;Based on the NBitWonder version (&lt;a href="http://nbitwonder.com"&gt;http://nbitwonder.com&lt;/a&gt;)
&lt;p&gt;&lt;strong&gt;Andrew Cooper&lt;/strong&gt;&lt;br&gt;28Nov2016&lt;br&gt;&lt;a href="http://www.darkerview.com"&gt;www.DarkerView.com&lt;/a&gt;</description>
<packages>
<package name="OSHW_8MM">
</package>
</packages>
</library>
<library name="Resistor_Axial">
<packages>
<package name="AXIAL-0.3">
<description>&lt;h3&gt;AXIAL-0.3&lt;/h3&gt;
&lt;p&gt;Commonly used for 1/4W through-hole resistors. 0.3" pitch between holes.&lt;/p&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="J2" library="SparkFun-Connectors" package="1X08" value="1X08">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CONN-08438"/>
<attribute name="VALUE"/>
</element>
<element name="U1" library="Teensy_LC" package="TEENSY_LC" value="TEENSY_LC"/>
<element name="J1" library="Zenith" package="ZENITH_CON" value="23-0039532245-ND">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="Resistor_Axial" package="AXIAL-0.3" value="75">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="Resistor_Axial" package="AXIAL-0.3" value="75">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="Resistor_Axial" package="AXIAL-0.3" value="75">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="Resistor_Axial" package="AXIAL-0.3" value="75">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$2" library="oshw" package="OSHW_8MM" value=""/>
</elements>
<signals>
<signal name="IO_0">
<contactref element="U1" pad="0"/>
<contactref element="J1" pad="P$18"/>
</signal>
<signal name="IO_22">
<contactref element="U1" pad="22"/>
<contactref element="J1" pad="P$17"/>
</signal>
<signal name="IO_1">
<contactref element="U1" pad="1"/>
<contactref element="J1" pad="P$16"/>
</signal>
<signal name="IO_2">
<contactref element="U1" pad="2"/>
<contactref element="J1" pad="P$15"/>
</signal>
<signal name="IO_21">
<contactref element="U1" pad="21"/>
<contactref element="R1" pad="P$1"/>
</signal>
<signal name="IO_3">
<contactref element="U1" pad="3"/>
<contactref element="J1" pad="P$14"/>
</signal>
<signal name="IO_4">
<contactref element="U1" pad="4"/>
<contactref element="J1" pad="P$12"/>
</signal>
<signal name="IO_20">
<contactref element="U1" pad="20"/>
<contactref element="J1" pad="P$11"/>
</signal>
<signal name="IO_5">
<contactref element="U1" pad="5"/>
<contactref element="R4" pad="P$1"/>
</signal>
<signal name="IO_19">
<contactref element="U1" pad="19"/>
<contactref element="J1" pad="P$10"/>
</signal>
<signal name="IO_6">
<contactref element="U1" pad="6"/>
<contactref element="J1" pad="P$9"/>
</signal>
<signal name="IO_18">
<contactref element="U1" pad="18"/>
<contactref element="J1" pad="P$8"/>
</signal>
<signal name="IO_7">
<contactref element="U1" pad="7"/>
<contactref element="J1" pad="P$7"/>
</signal>
<signal name="IO_17">
<contactref element="U1" pad="17"/>
<contactref element="R2" pad="P$1"/>
</signal>
<signal name="IO_8">
<contactref element="U1" pad="8"/>
<contactref element="J1" pad="P$6"/>
</signal>
<signal name="IO_16">
<contactref element="U1" pad="16"/>
<contactref element="R3" pad="P$1"/>
</signal>
<signal name="IO_9">
<contactref element="U1" pad="9"/>
<contactref element="J1" pad="P$5"/>
</signal>
<signal name="IO_15">
<contactref element="U1" pad="15"/>
<contactref element="J1" pad="P$4"/>
</signal>
<signal name="IO_10">
<contactref element="U1" pad="10"/>
<contactref element="J1" pad="P$3"/>
</signal>
<signal name="GND">
<contactref element="U1" pad="GND1"/>
<contactref element="U1" pad="GND2"/>
<contactref element="U1" pad="GND3"/>
<contactref element="J2" pad="4"/>
<contactref element="J1" pad="P$24"/>
</signal>
<signal name="IO_12">
<contactref element="J1" pad="P$1"/>
<contactref element="U1" pad="12"/>
</signal>
<signal name="13">
<contactref element="U1" pad="13"/>
<contactref element="J2" pad="2"/>
</signal>
<signal name="14">
<contactref element="U1" pad="14"/>
<contactref element="J2" pad="1"/>
</signal>
<signal name="26">
<contactref element="U1" pad="26"/>
<contactref element="J2" pad="3"/>
</signal>
<signal name="5V">
<contactref element="U1" pad="5V"/>
<contactref element="J2" pad="8"/>
</signal>
<signal name="3V">
<contactref element="U1" pad="3V2"/>
<contactref element="J2" pad="5"/>
</signal>
<signal name="IO_11">
<contactref element="J1" pad="P$2"/>
<contactref element="U1" pad="11"/>
</signal>
<signal name="PAD_LOCK">
<contactref element="J1" pad="P$22"/>
<contactref element="R1" pad="P$2"/>
</signal>
<signal name="CAPS_LOCK">
<contactref element="J1" pad="P$21"/>
<contactref element="R2" pad="P$2"/>
</signal>
<signal name="SCROLL_LOCK">
<contactref element="J1" pad="P$20"/>
<contactref element="R3" pad="P$2"/>
</signal>
<signal name="NUM_LOCK">
<contactref element="J1" pad="P$19"/>
<contactref element="R4" pad="P$2"/>
</signal>
<signal name="23">
<contactref element="U1" pad="23"/>
<contactref element="J2" pad="6"/>
</signal>
<signal name="24">
<contactref element="U1" pad="24"/>
<contactref element="J2" pad="7"/>
</signal>
<signal name="IO_25">
<contactref element="U1" pad="25"/>
<contactref element="J1" pad="P$13"/>
</signal>
<signal name="3VLED">
<contactref element="U1" pad="3V1"/>
<contactref element="J1" pad="P$23"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
