<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.5.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="17" y2="0" width="0" layer="20"/>
<wire x1="17" y1="0" x2="17" y2="17.7" width="0" layer="20"/>
<wire x1="17" y1="17.7" x2="0" y2="17.7" width="0" layer="20"/>
<wire x1="0" y1="17.7" x2="0" y2="0" width="0" layer="20"/>
<hole x="8.8" y="15.1" drill="2.8"/>
<text>2</text>
<text>3</text>
<text>4</text>
<text>5</text>
<text>6</text>
<text>7</text>
<text>8</text>
<text>1</text>
<text>GND</text>
<text>Gate</text>
<text>Drain</text>
<text>1mm pitch</text>
<text>MMBF170</text>
<text>G</text>
<text>D</text>
<text>S</text>
<text>1206</text>
</plain>
<libraries>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Connectors&lt;/h3&gt;
This library contains electrically-functional connectors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X01">
<description>&lt;h3&gt;Plated Through Hole&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:1&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_01&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="2X4">
<description>&lt;h3&gt;Plated Through Hole - 2x4&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:8&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_04x2&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="MMBF170">
<packages>
<package name="MMBF170">
</package>
</packages>
</library>
<library name="R1206">
<packages>
<package name="R1206">
</package>
</packages>
</library>
<library name="522710879">
<packages>
<package name="522710879">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="Q1" library="MMBF170" package="MMBF170" value="MMBF170">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="R1206" package="R1206" value="1206">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J3" library="SparkFun-Connectors" package="1X01" value="J3">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J4" library="SparkFun-Connectors" package="1X01" value="J4">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J5" library="SparkFun-Connectors" package="1X01" value="J5">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J1" library="522710879" package="522710879" value="j1">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J2" library="SparkFun-Connectors" package="2X4" value="j2">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="Q1" pad="2"/>
<contactref element="J5" pad="1"/>
<contactref element="J1" pad="P$9"/>
<contactref element="J1" pad="P$10"/>
</signal>
<signal name="N$11">
<contactref element="Q1" pad="3"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="N$12">
<contactref element="R1" pad="2"/>
<contactref element="J3" pad="1"/>
</signal>
<signal name="N$13">
<contactref element="J4" pad="1"/>
<contactref element="Q1" pad="1"/>
</signal>
<signal name="N$6">
<contactref element="J2" pad="6"/>
<contactref element="J1" pad="P$6"/>
</signal>
<signal name="N$8">
<contactref element="J2" pad="8"/>
<contactref element="J1" pad="P$8"/>
</signal>
<signal name="N$7">
<contactref element="J2" pad="7"/>
<contactref element="J1" pad="P$7"/>
</signal>
<signal name="N$5">
<contactref element="J2" pad="5"/>
<contactref element="J1" pad="P$5"/>
</signal>
<signal name="N$4">
<contactref element="J2" pad="4"/>
<contactref element="J1" pad="P$4"/>
</signal>
<signal name="N$3">
<contactref element="J2" pad="3"/>
<contactref element="J1" pad="P$3"/>
</signal>
<signal name="N$2">
<contactref element="J2" pad="2"/>
<contactref element="J1" pad="P$2"/>
</signal>
<signal name="N$1">
<contactref element="J2" pad="1"/>
<contactref element="J1" pad="P$1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
