<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="55" y2="0" width="0" layer="20"/>
<wire x1="55" y1="0" x2="55" y2="70" width="0" layer="20"/>
<wire x1="55" y1="70" x2="0" y2="70" width="0" layer="20"/>
<wire x1="0" y1="70" x2="0" y2="54.8" width="0" layer="20"/>
<hole x="3.5" y="66.5" drill="2.75"/>
<hole x="3.5" y="3.5" drill="2.75"/>
<hole x="51.5" y="3.5" drill="2.75"/>
<hole x="51.5" y="66.5" drill="2.75"/>
<wire x1="0" y1="36.6" x2="0" y2="0" width="0" layer="20"/>
<wire x1="0" y1="36.6" x2="36.3" y2="36.6" width="0" layer="20"/>
<wire x1="36.3" y1="36.6" x2="36.3" y2="54.8" width="0" layer="20"/>
<wire x1="36.3" y1="54.8" x2="0" y2="54.8" width="0" layer="20"/>
<text>VIN</text>
<text>AGND</text>
<text>3V</text>
<text>23</text>
<text>22</text>
<text>21</text>
<text>20</text>
<text>19</text>
<text>18</text>
<text>17</text>
<text>16</text>
<text>15</text>
<text>14</text>
<text>13</text>
<text>GND</text>
<text>0</text>
<text>1</text>
<text>2</text>
<text>3</text>
<text>4</text>
<text>5</text>
<text>6</text>
<text>7</text>
<text>8</text>
<text>9</text>
<text>10</text>
<text>11</text>
<text>12</text>
<text>24</text>
<text>25</text>
<text>26</text>
<text>27</text>
<text>33</text>
<text>28</text>
<text>32</text>
<text>31</text>
<text>30</text>
<text>29</text>
<text>1mm</text>
<text>0.8mm</text>
<text>0.5mm</text>
<text>Teensy 3.2
Low Profile
FPC Connector
Board</text>
</plain>
<libraries>
<library name="FPC34">
<packages>
<package name="FPC34">
</package>
</packages>
</library>
<library name="FPC34_p8mm">
<packages>
<package name="FPC34_P8MM">
</package>
</packages>
</library>
<library name="FPC34_p5mm">
<packages>
<package name="FPC34_P5MM">
</package>
</packages>
</library>
<library name="TEENSY3P2CUTOUT">
<packages>
<package name="TEENSY3P2CUTOUT">
</package>
</packages>
</library>
<library name="oshw">
<description>&lt;p&gt;&lt;strong&gt;Open Source Hardware PCB Logos&lt;/strong&gt;
&lt;p&gt;A simple polygon based version of the OSHWA logos for use on Eagle PCB's
&lt;p&gt;For use please refer to the OSHWA definition at &lt;a href="http://www.oshwa.org/definition/"&gt;http://www.oshwa.org/definition/&lt;/a&gt;
&lt;p&gt;Based on the NBitWonder version (&lt;a href="http://nbitwonder.com"&gt;http://nbitwonder.com&lt;/a&gt;)
&lt;p&gt;&lt;strong&gt;Andrew Cooper&lt;/strong&gt;&lt;br&gt;28Nov2016&lt;br&gt;&lt;a href="http://www.darkerview.com"&gt;www.DarkerView.com&lt;/a&gt;</description>
<packages>
<package name="OSHW_8MM">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="J1" library="FPC34" package="FPC34" value="1mm">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J2" library="FPC34_p8mm" package="FPC34_P8MM" value="0.8mm">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J3" library="FPC34_p5mm" package="FPC34_P5MM" value="0.5mm">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U1" library="TEENSY3P2CUTOUT" package="TEENSY3P2CUTOUT" value="Teensy 3.2">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$1" library="oshw" package="OSHW_8MM" value=""/>
</elements>
<signals>
<signal name="0">
<contactref element="U1" pad="0"/>
<contactref element="J1" pad="2"/>
<contactref element="J2" pad="2"/>
<contactref element="J3" pad="2"/>
</signal>
<signal name="1">
<contactref element="U1" pad="1"/>
<contactref element="J1" pad="4"/>
<contactref element="J2" pad="4"/>
<contactref element="J3" pad="4"/>
</signal>
<signal name="2">
<contactref element="U1" pad="2"/>
<contactref element="J1" pad="6"/>
<contactref element="J2" pad="6"/>
<contactref element="J3" pad="6"/>
</signal>
<signal name="3">
<contactref element="U1" pad="3"/>
<contactref element="J1" pad="8"/>
<contactref element="J2" pad="8"/>
<contactref element="J3" pad="8"/>
</signal>
<signal name="4">
<contactref element="U1" pad="4"/>
<contactref element="J1" pad="10"/>
<contactref element="J2" pad="10"/>
<contactref element="J3" pad="10"/>
</signal>
<signal name="5">
<contactref element="U1" pad="5"/>
<contactref element="J1" pad="12"/>
<contactref element="J2" pad="12"/>
<contactref element="J3" pad="12"/>
</signal>
<signal name="6">
<contactref element="U1" pad="6"/>
<contactref element="J1" pad="14"/>
<contactref element="J2" pad="14"/>
<contactref element="J3" pad="14"/>
</signal>
<signal name="7">
<contactref element="U1" pad="7"/>
<contactref element="J1" pad="16"/>
<contactref element="J2" pad="16"/>
<contactref element="J3" pad="16"/>
</signal>
<signal name="8">
<contactref element="U1" pad="8"/>
<contactref element="J1" pad="18"/>
<contactref element="J2" pad="18"/>
<contactref element="J3" pad="18"/>
</signal>
<signal name="9">
<contactref element="U1" pad="9"/>
<contactref element="J1" pad="20"/>
<contactref element="J2" pad="20"/>
<contactref element="J3" pad="20"/>
</signal>
<signal name="10">
<contactref element="U1" pad="10"/>
<contactref element="J1" pad="22"/>
<contactref element="J2" pad="22"/>
<contactref element="J3" pad="22"/>
</signal>
<signal name="11">
<contactref element="U1" pad="11"/>
<contactref element="J1" pad="24"/>
<contactref element="J2" pad="24"/>
<contactref element="J3" pad="24"/>
</signal>
<signal name="12">
<contactref element="U1" pad="12"/>
<contactref element="J1" pad="26"/>
<contactref element="J2" pad="26"/>
<contactref element="J3" pad="26"/>
</signal>
<signal name="13">
<contactref element="U1" pad="13"/>
<contactref element="J1" pad="34"/>
<contactref element="J2" pad="34"/>
<contactref element="J3" pad="34"/>
</signal>
<signal name="14">
<contactref element="U1" pad="14"/>
<contactref element="J1" pad="33"/>
<contactref element="J2" pad="33"/>
<contactref element="J3" pad="33"/>
</signal>
<signal name="15">
<contactref element="U1" pad="15"/>
<contactref element="J1" pad="32"/>
<contactref element="J2" pad="32"/>
<contactref element="J3" pad="32"/>
</signal>
<signal name="16">
<contactref element="U1" pad="16"/>
<contactref element="J1" pad="31"/>
<contactref element="J2" pad="31"/>
<contactref element="J3" pad="31"/>
</signal>
<signal name="17">
<contactref element="U1" pad="17"/>
<contactref element="J1" pad="13"/>
<contactref element="J2" pad="13"/>
<contactref element="J3" pad="13"/>
</signal>
<signal name="18">
<contactref element="U1" pad="18"/>
<contactref element="J1" pad="11"/>
<contactref element="J2" pad="11"/>
<contactref element="J3" pad="11"/>
</signal>
<signal name="19">
<contactref element="U1" pad="19"/>
<contactref element="J1" pad="9"/>
<contactref element="J2" pad="9"/>
<contactref element="J3" pad="9"/>
</signal>
<signal name="20">
<contactref element="U1" pad="20"/>
<contactref element="J1" pad="7"/>
<contactref element="J2" pad="7"/>
<contactref element="J3" pad="7"/>
</signal>
<signal name="21">
<contactref element="U1" pad="21"/>
<contactref element="J1" pad="5"/>
<contactref element="J2" pad="5"/>
<contactref element="J3" pad="5"/>
</signal>
<signal name="22">
<contactref element="U1" pad="22"/>
<contactref element="J1" pad="3"/>
<contactref element="J2" pad="3"/>
<contactref element="J3" pad="3"/>
</signal>
<signal name="24">
<contactref element="U1" pad="24"/>
<contactref element="J1" pad="15"/>
<contactref element="J2" pad="15"/>
<contactref element="J3" pad="15"/>
</signal>
<signal name="25">
<contactref element="U1" pad="25"/>
<contactref element="J1" pad="17"/>
<contactref element="J2" pad="17"/>
<contactref element="J3" pad="17"/>
</signal>
<signal name="26">
<contactref element="U1" pad="26"/>
<contactref element="J1" pad="21"/>
<contactref element="J2" pad="21"/>
<contactref element="J3" pad="21"/>
</signal>
<signal name="27">
<contactref element="U1" pad="27"/>
<contactref element="J1" pad="23"/>
<contactref element="J2" pad="23"/>
<contactref element="J3" pad="23"/>
</signal>
<signal name="28">
<contactref element="U1" pad="28"/>
<contactref element="J1" pad="25"/>
<contactref element="J2" pad="25"/>
<contactref element="J3" pad="25"/>
</signal>
<signal name="32">
<contactref element="U1" pad="32"/>
<contactref element="J1" pad="27"/>
<contactref element="J2" pad="27"/>
<contactref element="J3" pad="27"/>
</signal>
<signal name="33">
<contactref element="U1" pad="33"/>
<contactref element="J1" pad="19"/>
<contactref element="J2" pad="19"/>
<contactref element="J3" pad="19"/>
</signal>
<signal name="GND">
<contactref element="U1" pad="GND"/>
</signal>
<signal name="29">
<contactref element="U1" pad="29"/>
<contactref element="J1" pad="30"/>
<contactref element="J2" pad="30"/>
<contactref element="J3" pad="30"/>
</signal>
<signal name="30">
<contactref element="U1" pad="30"/>
<contactref element="J1" pad="29"/>
<contactref element="J2" pad="29"/>
<contactref element="J3" pad="29"/>
</signal>
<signal name="31">
<contactref element="U1" pad="31"/>
<contactref element="J1" pad="28"/>
<contactref element="J2" pad="28"/>
<contactref element="J3" pad="28"/>
</signal>
<signal name="23">
<contactref element="U1" pad="23"/>
<contactref element="J1" pad="1"/>
<contactref element="J2" pad="1"/>
<contactref element="J3" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
